#

### Sustainable Public Procurement-fiche: basic - 2010

# *1) Subject matter*

Indoor furniture produced with environmentally friendly materials and processes.

“For <…..> (name of the public authority), the care for the environment and social aspects is important. It is stated in her <strategic policies>, <mission>, <vision>, <procurement policy>, …”

***2) Exclusion criteria***

Non compliance with environmental and social legislation, which has been the subject of a final judgment or a decision having equivalent effect, may be considered an offence concerning the professional conduct of the economic operator concerned or grave misconduct, permitting to exclude the party concerned from competing for the contract

Ref:

Art. 53 and 54 of Directive 2004/17/EC and Art. 45 of Directive 2004/18/EC

***3) Technical capacity***

***/***

***4) Technical specifications***

***General***

* The VOC content of adhesives used in the assembly of furniture do not exceed 10% by weight [Eu toolkit core criteria]

***Wood and wood-based materials***

- All wood and wood-based materials come from legally sourced timber and is traceable. The wood material shall not come from forest environments that need protection for biological and/or social reasons. When the wood is certified as FSC, PEFC or any other equivalent means of proof, this will be accepted as proof of compliance. [EU toolkit core criteria]

***Surface coating of wood, plastic and/or metal parts***

* The products used for coating shall:
	+ Not contain hazardous substances that are classified according to Directive 1999/45/EC as carcinogenic (R40, R45, R49), harmful to the reproductive system (R60, R61, R62, R63), mutagenic (R46, R68), toxic (R23, R24, R25, R26, R27, R28, R51), allergenic when inhaled (R42) or harmful to the environment (R50, R50/53, R51/53, R52, R52/53, R53). Cause heritable genetic damage (R46), danger of serious damage to health by prolonged exposure (R48), possible risks of irreversible effects (R68). For phthalates: No use is allowed of phthalates that at the time of application fulfil the classification criteria of any of the following risk phrases (or combinations thereof): R60, R61, R62, in accordance with Directive 67/548/EEC and its amendments. [EU toolkit core criteria]
	+ Not contain aziridine [EU toolkit core criteria]
	+ Not contain Chromium (VI) compounds [EU toolkit core criteria]
	+ Not contain more than 5% by weight of volatile organic compounds [EU toolkit core criteria]

***Plastic parts***

All plastic parts ≥ 50g shall be marked for recycling according to ISO 11469 or equivalent and must not contain additions of other materials that may hinder their recycling. [EU toolkit core criteria]

 ***Packaging materials***

* Packaging must consist of readily recycled material, and/or materials taken from renewable resources, or be a multi-use system. [EU toolkit core criteria]
* All packaging materials shall be easily separable by hand into recyclable parts consisting of one material (e.g. cardboard, paper, plastic, textile). [EU toolkit core criteria]

***Evidence:***

The compliance with all the criteria mentioned above can be proved with one of the following labels:

Nordic Swan Milieukeur NF Environnement

Labeling

in case that the tendering company can present one of these labels, any further proof is not necessary. Any other suitable evidence from a recognized body can also be used.

For the criteria of wood, compliance can also be proved by these labels:


## Blaue Engel FSC-label PEFC-label

## 5) Awarding the contract:

|  |  |  |
| --- | --- | --- |
|  | ***Criterium*** | ***Weight*** |
|  |  |  |
| 1 | ***Price*** *Calculation (e.g.):* Lowest offered price/ stated price x 0,70 | e.g. 70% |
| 2 | ***Environmental criteria***(The public authority formulates the points it wants to assign to the below mentioned criteria ) *Calculation (e.g.):* Total scored points / maximum number of points x 0,20 | e.g. 20% |
| 3 | … | e.g. 5 % |
| 4 | … | e.g. …. |

***Environmental criteria***

***General***

Maintenance of the tools is possible without the use of organic solvents.

 ***Wood***

***Raw material***

* The proportion of the wood that comes from sustainable forestry has to be indicated by the supplier. The higher this proportion the more awarding points that product receives. [EU toolkit core criteria]

***Plastics***

***Raw materials***

* Percentage by weight of the plastics that exist of postconsumer recycled material.The higher this percentage the more awarding point this product receives. [EU toolkit core criteria]
* It is possible to separate plastic parts from other materials (metals, wood or other types of plastics) without use of special tools.

***Surface treatment of plastics***

The plastic parts are not surface treated.

***Metals***

***Raw materials***

- Percentage by weight of the metals that exists of postconsumer recycled material.The higher this percentage the more awarding point this product receives. [EU toolkit core criteria]

- It is possible to separate the metal from other materials in the product (does not include surface treatment) without use of special tools.

***Textile (also synthetic fibers)***

The criteria with regard to textile can be found in the category ‘Clothing and accessories’ (http://www.gidsvoorduurzameaankopen.be/?q=en/node/47&cid=153&pid=1285)

***Leather***

* The criteria with regard to leather can be found in the category ‘Leather products’ (http://www.gidsvoorduurzameaankopen.be/?q=en/node/47&cid=153&pid=1289)

***Polyurethane***

* Partially fluorinated hydrocarbons (HFCs), , partially halogenated chlorofluorocarbons (H-CFC), chlorofluorocarbons (CFCs) or methylene chloride are not used as physical blowing agents or auxiliary blowing agents in the production of polyurethane foam (PUR). [EU toolkit core criteria]

***Stony materials***

* If nature stone is used, this comes from a quarry for what is made up a landscape recovery plan based on an environmental effect rapport conform EU directive 85/337 or an equal environmental study.

***Recyclability***

* It is possible to separate 90% of the parts from metal, wood, plastic and inert materials from the other materials without the use of special tools. Panel materials with plastic or synthetical resin do not have to be separatable.
* For upholstered furniture:
	+ if the upholstery is fixed to the basic construction then it has to be easy to separate it from this construction. This means that glue surfaces that can not be easily detached are not allowed, joints with clips are allowed for joints that can be used in new parts.
	+ if the upholstery is integrated with a part of the seat and/or the back it has to be easy to separated both. Glue, screw and nail joints who can not be easily detached are not allowed, weld and melt joints are not allowed. Connections with clips are allowed for connections that can be used in new parts.

***6) Performance clauses:***

.

***Guarantee and spare parts:***

* The supplier maintains separately access to spare parts of the furniture (as hinges and weels) for at least 10 years after the delivery of the tool.
* By normal use and maintenance a life time of 5 years has to be guaranteed.

###  References

[Information of the public authority that used these clauses in a procurement case]

**Annex R-PHRASES:**

**(R-phrases are mentioned on product labels and in product safety datasheets. It can be a useful tool for verification-procedures.)**

|  |  |
| --- | --- |
| [R1](http://www.umwelt-online.de:80/regelwerk/eu/65_69/an6a.htm#r1): | Explosive when dry. |
| [R2](http://www.umwelt-online.de:80/regelwerk/eu/65_69/an6a.htm#r2): | Risk of explosion by shock, friction, fire or other sources of ignition. |
| [R3](http://www.umwelt-online.de:80/regelwerk/eu/65_69/an6a.htm#r3): | Extreme risk of explosion by shock, friction, fire or other sources of ignition. |
| [R4](http://www.umwelt-online.de:80/regelwerk/eu/65_69/an6a.htm#r4): | Forms very sensitive explosive metallic compounds. |
| [R5](http://www.umwelt-online.de:80/regelwerk/eu/65_69/an6a.htm#r5): | Heating may cause an explosion. |
| [R6](http://www.umwelt-online.de:80/regelwerk/eu/65_69/an6a.htm#r6): | Explosive with or without contact with air. |
| [R7](http://www.umwelt-online.de:80/regelwerk/eu/65_69/an6a.htm#r7): | May cause fire. |
| [R8](http://www.umwelt-online.de:80/regelwerk/eu/65_69/an6a.htm#r8): | Contact with combustible material may cause fire. |
| [R9](http://www.umwelt-online.de:80/regelwerk/eu/65_69/an6a.htm#r9): | Explosive when mixed with combustible material. |
| [R10](http://www.umwelt-online.de:80/regelwerk/eu/65_69/an6a.htm#r10): | Flammable |
| [R11](http://www.umwelt-online.de:80/regelwerk/eu/65_69/an6a.htm#r11): | Highly flammable |
| [R12](http://www.umwelt-online.de:80/regelwerk/eu/65_69/an6a.htm#r12): | Extremely flammable |
| *R13 (obsolet):* | *Extremely flammable liquid gas**(This R-phrase is no longer designated by the version of  the GefStoffV published on 26.10.93.)* |
| [R14](http://www.umwelt-online.de:80/regelwerk/eu/65_69/an6a.htm#r14): | Reacts violently with water. |
| [R15](http://www.umwelt-online.de:80/regelwerk/eu/65_69/an6a.htm#r15): | Contact with water liberates extremely flammable gases. |
| *Merck R15.1* | *Contact with acid liberates extremely flammable gases.* |
| [R16](http://www.umwelt-online.de:80/regelwerk/eu/65_69/an6a.htm#r16): | Explosive when mixed with oxidizing substances. |
| [R17](http://www.umwelt-online.de:80/regelwerk/eu/65_69/an6a.htm#r17): | Spontaneously flammable in air. |
| [R18](http://www.umwelt-online.de:80/regelwerk/eu/65_69/an6a.htm#r18): | In use, may form flammable/explosive vapour-air mixture. |
| [R19](http://www.umwelt-online.de:80/regelwerk/eu/65_69/an6a.htm#r19): | May form explosive peroxides. |
| [R20](http://www.umwelt-online.de:80/regelwerk/eu/65_69/an6b.htm#r20): | Harmful by inhalation. |
| [R21](http://www.umwelt-online.de:80/regelwerk/eu/65_69/an6b.htm#r21): | Harmful in contact with skin. |
| [R22](http://www.umwelt-online.de:80/regelwerk/eu/65_69/an6b.htm#r22): | Harmful if swallowed. |
| [R23](http://www.umwelt-online.de:80/regelwerk/eu/65_69/an6b.htm#r23): | Toxic by inhalation. |
| *Riedel-de Haen* *R23K:* | *Also toxic by inhalation.* |
| [R24](http://www.umwelt-online.de:80/regelwerk/eu/65_69/an6b.htm#r24): | Toxic in contact with skin. |
| *Riedel-de Haen* *R24K:* | *Also toxic in contact with skin.* |
| [R25](http://www.umwelt-online.de:80/regelwerk/eu/65_69/an6b.htm#r25): | Toxic if swallowed. |
| *Riedel-de Haen* *R25K:* | *Also toxic if swallowed.* |
| [R26](http://www.umwelt-online.de:80/regelwerk/eu/65_69/an6b.htm#r26): | Very toxic by inhalation. |
| *Riedel-de Haen* *R26K:* | *Also very toxic by inhalation.* |
| [R27](http://www.umwelt-online.de:80/regelwerk/eu/65_69/an6b.htm#r27): | Very toxic in contact with skin |
| *Riedel-de Haen* *R27A:* | *Very toxic in contact with eyes.* |
| *Riedel-de Haen* *R27K:* | *Also very toxic in contact with skin.* |
| *Riedel-de Haen* *R27AK:* | *Also very toxic in contact with eyes.* |
| [R28](http://www.umwelt-online.de:80/regelwerk/eu/65_69/an6b.htm#r28): | Very toxic if swallowed. |
| *Riedel-de Haen* *R28K:* | *Also very toxic if swallowed.* |
| [R29](http://www.umwelt-online.de:80/regelwerk/eu/65_69/an6c.htm#r29): | Contact with water liberates toxic gas. |
| [R30](http://www.umwelt-online.de:80/regelwerk/eu/65_69/an6a.htm#r30): | Can become highly flammable in use. |
| [R31](http://www.umwelt-online.de:80/regelwerk/eu/65_69/an6c.htm#r31): | Contact with acids liberates toxic gas. |
| *Merck R31.1* | *Contact with alkalies liberates toxic gas.* |
| [R32](http://www.umwelt-online.de:80/regelwerk/eu/65_69/an6c.htm#r32): | Contact with acids liberates very toxic gas. |
| [R33](http://www.umwelt-online.de:80/regelwerk/eu/65_69/an6c.htm#r33): | Danger of cumulative effects. |
| [R34](http://www.umwelt-online.de:80/regelwerk/eu/65_69/an6b.htm#r34): | Causes burns. |
| [R35](http://www.umwelt-online.de:80/regelwerk/eu/65_69/an6b.htm#r35): | Causes severe burns. |
| [R36](http://www.umwelt-online.de:80/regelwerk/eu/65_69/an6b.htm#r36): | Irritating to eyes. |
| *Riedel-de Haen* *R36A:* | *Lacrimating* |
| R37: | Irritating to respiratory system. |
| [R38](http://www.umwelt-online.de:80/regelwerk/eu/65_69/an6b.htm#r38): | Irritating to skin. |
| [R39](http://www.umwelt-online.de:80/regelwerk/eu/65_69/an6b.htm#r39): | Danger of very serious irreversible effects. |
| [R40](http://www.umwelt-online.de:80/regelwerk/eu/65_69/an6c.htm#r40): | Possible risk of cancer.*CAUTION: Until 2001 this R-phrase was used for possible mutagenic or teratogenic risks as well. These risks are now labelled with R68!* |
| [R41](http://www.umwelt-online.de:80/regelwerk/eu/65_69/an6b.htm#r41): | Risk of serious damage to eyes. |
| [R42](http://www.umwelt-online.de:80/regelwerk/eu/65_69/an6c.htm#r42): | May cause sensitization by inhalation. |
| [R43](http://www.umwelt-online.de:80/regelwerk/eu/65_69/an6c.htm#r43): | May cause sensitization by skin contact. |
| [R44](http://www.umwelt-online.de:80/regelwerk/eu/65_69/an6a.htm#r44): | Risk of explosion if heated under confinement. |
| [R45](http://www.umwelt-online.de:80/regelwerk/eu/65_69/an6c.htm#r45): | May cause cancer. |
| [R46](http://www.umwelt-online.de:80/regelwerk/eu/65_69/an6c.htm#r46): | May cause heritable genetic damage. |
| *R47(obsolet):* | *May cause deformities.**(This R-phrase is no longer designated by the version of  the GefStoffV published on 26.10.93.)* |
| [R48](http://www.umwelt-online.de:80/regelwerk/eu/65_69/an6b.htm#r48): | Danger of serious damage to health by prolonged exposure. |
| [R49](http://www.umwelt-online.de:80/regelwerk/eu/65_69/an6c.htm#r49): | May cause cancer by inhalation. |
| [R50](http://www.umwelt-online.de:80/regelwerk/eu/65_69/an6d.htm#r50): | Very toxic to aquatic organisms. |
| [R51](http://www.umwelt-online.de:80/regelwerk/eu/65_69/an6d.htm#r51): | Toxic to aquatic organisms. |
| [R52](http://www.umwelt-online.de:80/regelwerk/eu/65_69/an6d.htm#r52): | Harmful to aquatic organisms. |
| [R53](http://www.umwelt-online.de:80/regelwerk/eu/65_69/an6d.htm#r53): | May cause long-term adverse effects in the aquatic environment. |
| [R54](http://www.umwelt-online.de:80/regelwerk/eu/65_69/an6d.htm#r54): | Toxic to flora. |
| [R55](http://www.umwelt-online.de:80/regelwerk/eu/65_69/an6d.htm#r55): | Toxic to fauna. |
| [R56](http://www.umwelt-online.de:80/regelwerk/eu/65_69/an6d.htm#r56): | Toxic to soil organisms. |
| [R57](http://www.umwelt-online.de:80/regelwerk/eu/65_69/an6d.htm#r57): | Toxic to bees. |
| [R58](http://www.umwelt-online.de:80/regelwerk/eu/65_69/an6d.htm#r58): | May cause long-term adverse effects in the environment. |
| [R59](http://www.umwelt-online.de:80/regelwerk/eu/65_69/an6e.htm#r59): | Dangerous for the ozone layer. |
| [R60](http://www.umwelt-online.de:80/regelwerk/eu/65_69/an6d.htm#r60): | May impair fertility. |
| [R61](http://www.umwelt-online.de:80/regelwerk/eu/65_69/an6d.htm#r61): | May cause harm to the unborn child. |
| [R62](http://www.umwelt-online.de:80/regelwerk/eu/65_69/an6d.htm#r62): | Possible risk of impaired fertility. |
| [R63](http://www.umwelt-online.de:80/regelwerk/eu/65_69/an6d.htm#r63): | Possible risk of harm to the unborn child. |
| [R64](http://www.umwelt-online.de:80/regelwerk/eu/65_69/an6c.htm#r64): | May cause harm to breastfed babies. |
| [R65:](http://www.umwelt-online.de:80/regelwerk/eu/65_69/an6b.htm#r65) | Harmful: may cause lung damage if swallowed. |
| [R66:](http://www.umwelt-online.de:80/regelwerk/eu/65_69/an6c.htm#r66) | Repeated exposure may cause skin dryness or cracking. |
| [R67:](http://www.umwelt-online.de:80/regelwerk/eu/65_69/an6c.htm#r67) | Vapours may cause drowsiness and dizziness. |
| [R68:](http://www.umwelt-online.de:80/regelwerk/eu/65_69/an6b.htm#r68) | Possible risks of irreversible effects. |

**COMBINATIONS OF R-PHRASES:**

|  |  |
| --- | --- |
| R14/15: | Reacts violently with water, liberating extremely flammable gases. |
| R15/29: | Contact with water liberates toxic, extremely flammable gas. |
| R20/21: | Harmful by inhalation and in contact with skin. |
| R21/22: | Harmful in contact with skin and if swallowed. |
| R20/22: | Harmful by inhalation and if swallowed. |
| R20/21/22: | Harmful by inhalation, in contact with skin and if swallowed. |
| R21/22: | Harmful in contact with skin and if swallowed. |
| R23/24: | Toxic by inhalation and in contact with skin. |
| R24/25: | Toxic in contact with skin and if swallowed. |
| R23/25: | Toxic by inhalation and if swallowed. |
| R23/24/25: | Toxic by inhalation, in contact with skin and if swallowed. |
| R24/25: | Toxic in contact with skin and if swallowed. |
| R26/27: | Very toxic by inhalation and in contact with skin. |
| R27/28: | Very toxic in contact with skin and if swallowed. |
| R26/28: | Very toxic by inhalation and if swallowed. |
| R26/27/28: | Very toxic by inhalation, in contact with skin and if swallowed. |
| R36/37: | Irritating to eyes and respiratory system. |
| R37/38: | Irritating to respiratory system and skin. |
| R36/38: | Irritating to eyes and skin. |
| R36/37/38: | Irritating to eyes, respiratory system and skin. |
| R39/23: | Toxic: danger of very serious irreversible effects through inhalation. |
| R39/24: | Toxic: danger of very serious irreversible effects in contact with skin. |
| R39/25: | Toxic: danger of very serious irreversible effects if swallowed. |
| R39/23/24: | Toxic: danger of very serious irreversible effects through inhalation and in contact with skin. |
| R39/23/25: | Toxic: danger of very serious irreversible effects through inhalation and if swallowed. |
| R39/24/25: | Toxic: danger of very serious irreversible effects in contact with skin and if swallowed. |
| R39/23/24/25: | Toxic: danger of very serious irreversible effects through inhalation, in contact with skin and if swallowed. |
| R39/26: | Very toxic: danger of very serious irreversible effects through inhalation. |
| R39/27: | Very toxic: danger of very serious irreversible effects in contact with skin. |
| R39/28: | Very toxic: danger of very serious irreversible effects if swallowed. |
| R39/26/27: | Very toxic: danger of very serious irreversible effects through inhalation and in contact with skin. |
| R39/26/28: | Very toxic: danger of very serious irreversible effects through inhalation and if swallowed. |
| R39/27/28: | Very toxic: danger of very serious irreversible effects in contact with skin and if swallowed. |
| R39/26/27/28: | Very toxic: danger of very serious irreversible effects through inhalation, in contact with skin and if swallowed. |
| R42/43: | May cause sensitization by inhalation and skin contact. |
| R48/20: | Harmful: danger of serious damage to health by prolonged exposure through inhalation. |
| R48/21: | Harmful: danger of serious damage to health by prolonged exposure in contact with skin. |
| R48/22: | Harmful: danger of serious damage to health by prolonged exposure if swallowed. |
| R48/20/21: | Harmful: danger of serious damage to health by prolonged exposure through inhalation and in contact with skin. |
| R48/20/22: | Harmful: danger of serious damage to health by prolonged exposure through inhalation and if swallowed. |
| R48/21/22: | Harmful: danger of serious damage to health by prolonged exposure in contact with skin and if swallowed. |
| R48/20/21/22: | Harmful: danger of serious damage to health by prolonged exposure through inhalation, in contact with skin and if swallowed. |
| R48/23: | Toxic: danger of serious damage to health by prolonged exposure through inhalation. |
| R48/24: | Toxic: danger of serious damage to health by prolonged exposure in contact with skin. |
| R48/25: | Toxic: danger of serious damage to health by prolonged exposure if swallowed. |
| R48/23/24: | Toxic: danger of serious damage to health by prolonged exposure through inhalation and in contact with skin. |
| R48/23/25: | Toxic: danger of serious damage to health by prolonged exposure through inhalation and if swallowed. |
| R48/24/25: | Toxic: danger of serious damage to health by prolonged exposure in contact with skin and if swallowed. |
| R48/23/24/25: | Toxic: danger of serious damage to health by prolonged exposure through inhalation, in contact with skin and if swallowed. |
| R50/53: | Very toxic to aquatic organisms, may cause long-term adverse effects in the aquatic environment. |
| R51/53: | Toxic to aquatic organisms, may cause long-term adverse effects in the aquatic environment. |
| R52/53: | Harmful to aquatic organisms, may cause long-term adverse effects in the aquatic environment. |
| R68/20: | Harmful: possible risk of irreversible effects through inhalation. |
| R68/21: | Harmful: possible risk of irreversible effects in contact with skin. |
| R68/22: | Harmful: possible risk of irreversible effects if swallowed. |
| R68/20/21: | Harmful: possible risk of irreversible effects through inhalation and in contact with skin. |
| R68/20/22: | Harmful: possible risk of irreversible effects through inhalation and if swallowed. |
| R68/21/22: | Harmful: possible risk of irreversible effects in contact with skin and if swallowed. |
| R68/20/21/22: | Harmful: possible risk of irreversible effects through inhalation, in contact with skin and if swallowed. |